**Lab - View the Switch MAC Address Table**

# Topology



# Addressing Table

| Device | Interface | IP Address | Subnet Mask |
| --- | --- | --- | --- |
| S1 | VLAN 1 | 192.168.1.11 | 255.255.255.0 |
| S2 | VLAN 1 | 192.168.1.12 | 255.255.255.0 |
| PC-A | NIC | 192.168.1.1 | 255.255.255.0 |
| PC-B | NIC | 192.168.1.2 | 255.255.255.0 |

# Objectives

Part 1: Build and Configure the Network

Part 2: Examine the Switch MAC Address Table

# Background / Scenario

The purpose of a Layer 2 LAN switch is to deliver Ethernet frames to host devices on the local network. The switch records host MAC addresses that are visible on the network, and maps those MAC addresses to its own Ethernet switch ports. This process is called building the MAC address table. When a switch receives a frame from a PC, it examines the frame’s source and destination MAC addresses. The source MAC address is recorded and mapped to the switch port from which it arrived. Then the destination MAC address is looked up in the MAC address table. If the destination MAC address is a known address, then the frame is forwarded out of the corresponding switch port associated with that MAC address. If the MAC address is unknown, then the frame is broadcasted out of all switch ports, except the one from which it came. It is important to observe and understand the function of a switch and how it delivers data on the network. The way a switch operates has implications for network administrators whose job it is to ensure secure and consistent network communication.

Switches are used to interconnect and deliver information to computers on local area networks. Switches deliver Ethernet frames to host devices identified by network interface card MAC addresses.

In Part 1, you will build a multi-switch topology with a trunk linking the two switches. In Part 2, you will ping various devices and observe how the two switches build their MAC address tables.

**Note**: The switches used are Cisco Catalyst 2960s with Cisco IOS Release 15.2(2) (lanbasek9 image). Other switches and Cisco IOS versions can be used. Depending on the model and Cisco IOS version, the commands available and output produced might vary from what is shown in the labs.

**Note**: Make sure that the switches have been erased and have no startup configurations. If you are unsure contact your instructor.

# Required Resources

* 2 Switches (Cisco 2960 with Cisco IOS Release 15.2(2) lanbasek9 image or comparable)
* 2 PCs (Windows with terminal emulation program, such as Tera Term)
* Console cables to configure the Cisco IOS devices via the console ports
* Ethernet cables as shown in the topology

**Note**: The Fast Ethernet interfaces on Cisco 2960 switches are autosensing and an Ethernet straight-through cable may be used between switches S1 and S2. If using another model Cisco switch, it may be necessary to use an Ethernet crossover cable.

# Instructions

## Build and Configure the Network

### Cable the network according to the topology.

A picture containing screenshot

Description automatically generated

### Configure PC hosts.

A screenshot of a computer

Description automatically generatedA screenshot of a computer

Description automatically generated

### Initialize and reload switches as necessary.

### Configure basic settings for each switch.

Open configuration window

* + - 1. Configure device name as shown in the topology.
      2. Configure IP address as listed in Addressing Table.
      3. Assign **cisco** as the console and vty passwords.
      4. Assign **class** as the privileged EXEC password.

Close configuration window

## Examine the Switch MAC Address Table

A switch learns MAC addresses and builds the MAC address table, as network devices initiate communication on the network.

### Record network device MAC addresses.

* + - 1. Open a command prompt on PC-A and PC-B and type **ipconfig /all**.

Open Windows command prompt

#### Question:

What are the Ethernet adapter physical addresses?

PC-A MAC Address:

00-50-56-B3-27-D6.

PC-B MAC Address:

00-50-56-B3-FF-54.

Close Windows command prompt

* + - 1. Console into switch S1 and S2 and type the **show interface F0/1** command on each switch.

Open a configuration window

#### Questions:

On the second line of command output, what is the hardware addresses (or burned-in address [bia])?

S1 Fast Ethernet 0/1 MAC Address:

0cd9.96e2.3d01.

S2 Fast Ethernet 0/1 MAC Address:

0cd9.96e2.3f81.

Close a configuration window

### Display the switch MAC address table.

Console into switch S2 and view the MAC address table, both before and after running network communication tests with ping.

* + - 1. Establish a console connection to S2 and enter privileged EXEC mode.

Open a configuration window

* + - 1. In privileged EXEC mode, type the **show mac address-table** command and press Enter.

S2# **show mac address-table**

Even though there has been no network communication initiated across the network (i.e., no use of ping), it is possible that the switch has learned MAC addresses from its connection to the PC and the other switch.

#### Questions:

Are there any MAC addresses recorded in the MAC address table?

Switch có thể có một hoặc nhiều địa chỉ MAC trong bảng của nó. Switch có thể đã học được địa chỉ MAC thông qua cổng chuyển đổi của S1. Công tắc sẽ ghi lại nhiều địa chỉ MAC của máy chủ đã học thông qua kết nối với công tắc khác.

What MAC addresses are recorded in the table? To which switch ports are they mapped and to which devices do they belong? Ignore MAC addresses that are mapped to the CPU.

Có thể có nhiều địa chỉ MAC được ghi trong bảng địa chỉ MAC, đặc biệt là các địa chỉ MAC được học thông qua cổng chuyển đổi của S1. Trong ví dụ đầu ra ở trên, địa chỉ MAC máy S1 và địa chỉ MAC PCA được ánh xạ tới máy S2.

If you had not previously recorded MAC addresses of network devices in Step 1, how could you tell which devices the MAC addresses belong to, using only the output from the **show mac address-table** command? Does it work in all scenarios?

Đầu ra của lệnh show mac address-table hiển thị cổng mà địa chỉ MAC đã tự học trên đó. Điều này sẽ xác định địa chỉ MAC thuộc về thiết bị mạng nào, ngoại trừ trường hợp nhiều địa chỉ MAC được liên kết với cùng một cổng. Điều này xảy ra khi các switch được kết nối với các switch khác và ghi lại tất cả địa chỉ MAC cho các thiết bị được kết nối với switch kia.

### Clear the S2 MAC address table and display the MAC address table again.

* + - 1. In privileged EXEC mode, type the **clear mac address-table dynamic** command and press **Enter**.

S2# **clear mac address-table dynamic**

* + - 1. Quickly type the **show mac address-table** command again.

#### Questions:

Does the MAC address table have any addresses in it for VLAN 1? Are there other MAC addresses listed?

Bảng địa chỉ MAC không có địa chỉ ở trong VLAN 1.

Wait 10 seconds, type the **show mac address-table** command, and press Enter. Are there new addresses in the MAC address table?

Có.

Close a configuration window

### From PC-B, ping the devices on the network and observe the switch MAC address table.

* + - 1. From PC-B, open a command prompt and type **arp -a**.

Open a command prompt

#### Question:

Not including multicast or broadcast addresses, how many device IP-to-MAC address pairs have been learned by ARP?

Có 4 thiết bị.

* + - 1. From the PC-B command prompt, ping PC-A, S1, and S2.

#### Question:

Did all devices have successful replies? If not, check your cabling and IP configurations.

Có.

Close a command prompt

* + - 1. From a console connection to S2, enter the **show mac address-table** command.

Open a configuration window

#### Question:

Has the switch added additional MAC addresses to the MAC address table? If so, which addresses and devices?

Switch chưa được add vào địa chỉ MAC trong bảng địa chỉ MAC.

Close a configuration window

Open a command prompt

From PC-B, open a command prompt and retype **arp -a**.

#### Question:

Does the PC-B ARP cache have additional entries for all network devices that were sent pings?

Có.

Close a command prompt

# Reflection Question

On Ethernet networks, data is delivered to devices by their MAC addresses. For this to happen, switches and PCs dynamically build ARP caches and MAC address tables. With only a few computers on the network this process seems fairly easy. What might be some of the challenges on larger networks?

Sóng ARP có thể gây ra các nhiễu đường truyền sóng. ARP và bảng MAC chuyển đổi không xác thực hoặc xác thực địa chỉ IP thành địa chỉ MAC.

End of Document